 

All-New Ford Ranger: Preliminary Technical Specifications 
Features

Structure
Computer-optimized, high-efficiency, unitary-welded steel, body on frame




Safety elements - Body
Optimized frame and body structure to achieve moderate deceleration levels whilst minimizing intrusions into the passenger compartment in offset and straight front impacts, side impacts and rear impacts.

Front end optimized for pedestrian protection, with energy absorbing material in the front bumper and 'hexageneous' under-bonnet structure



Passive safety and restraint system elements
Ford Intelligent Protection System (IPS) featuring:

· Full size driver and passenger airbags 

· Driver knee airbag 

· Standard inflatable side curtains for front and second row occupants

· Standard thorax-protecting side airbags for front occupants

· Three-point safety belts in all positions

· Safety belt reminders for driver & front passenger

· Safety belt pretensioners and load limiters for driver & front passenger

· Passenger airbag deactivation switch

· ISOFIX anchor points for the rear outer seats




Security system elements
· Thatcham Cat1 alarm with interior scanning capability, with Battery Back-up Sounder

· Advanced Ford PATS immobiliser

· Remote and manual key operated central locking



Corrosion protection
12 year anti-corrosion warranty.




Aerodynamics
Ranger Double Cab



CD: 040



A: 2.86 





Suspension
Front – Independent front suspension with coil-over-strut design 





Rear – Rigid leafs springs




Steering
Type – Rack and pinion steering, power assisted





Turning circle (m, Kerb-to-Kerb) – 11.8 (4x2); 12.4 (4x4)





Turns lock-to-lock – 3.5    




Brakes
Front – ventilated discs, 302 x 32mm




Rear – drums, 270 x 55mm (4x2); 295 x 55mm (4x4)




Modulation:

Standard: Electronic Stability Program (ESP), Traction Control System (TCS), Electronic Brake Assist.

ESP system features: Hill Descent Control (HDC), Hill Launch Assist (HLA), Trailer Sway Mitigation (TSM), Load Adaptive Control (LAC), Emergency Brake Assist (EBA), Emergency Brake Light (EBL), Roll-Over Mitigation (ROM)



Wheels & tyres

Wheel type

Pressed Steel 
Pressed Steel / Alloy 
Alloy
Alloy
Wheel size

6.5 x 16"

7.0 x 16"

8.0 x 17"

8.0 x 18"

Tyre size

215/70 R 16
255/55 R 16
265/65 R 17
265/60 R 18
Spare wheel:

16" full-size steel spare 

Engine Type
2.2L Duratorq TDCi 150 PS/120 kW 

Displacement (cc)
2198

Bore (mm)
86.0

Stroke (mm)
94.6

Fuel type, grade
Diesel GOPS A10 B10 Gazole EN590 with 10% of FAME EN14214

Max power (ISO kW/PS)
120/150

At engine speed (rpm)
3700

Max torque (ISO Nm)
375 

At engine speed (rpm)
1500-2500

Compression ratio
15.7:1

Cylinders
4 in line

Turbocharger
Variable Geometry Turbocharger with position sensor

Fuel injection
High-pressure common-rail with fuel pressure 1800bar 



Emission controls
Coated Diesel Particulate Filter (cDPF)

Oxidation catalyst

Emission level
Water cooled EGR

Euro Stage V

TRANSMISSION

Transmission type: 
Ford MT82 manual 6-speed 
Ford 6R80 automatic 6-speed 

Gear ratios 


6th

5th

4th

3rd 

2nd

1st

Reverse

Final Drive (4x2)

Final Drive (4x4)
0.794

0.691

1.000

0.867

1.223

1.143

1.721

1.521

2.839

2.342

5.441

4.171

4.935

3.400

3.31

3.55

-

3.73



Clutch
Hydraulically operated self-adjust clutch with dual mass flywheel
6-speed automatic transmission with manual Sport Mode, Brake Shift Interlock, Grade Control Logic (Automatic modes), Emergency downshift (Manual mode)

4x4 Transfer box
Two speed, right hand drop, single offset , aluminium shift-on-the-fly transfer box

4x4 ratios


1:1 (High Range)

2.48:1 (Low Range)

Max. speed when switching
120 km/h

Engine Type
3.2L Duratorq TDCi 200 PS/147 kW 

Displacement (cc)
3198

Bore (mm)
89.9

Stroke (mm)
100.76

Fuel type, grade
Diesel GOPS A10 B10 Gazole EN590 with 10% of FAME EN14214

Max power (ISO kW/PS)
147/200

At engine speed (rpm)
3000

Max torque (ISO Nm)
470 

At engine speed (rpm)
1500-2750

Compression ratio
15.7:1

Cylinders
5 in line

Turbocharger
Variable Geometry Turbocharger with position sensor

Fuel injection
High-pressure common-rail with fuel pressure 1800bar 



Emission controls
Coated Diesel Particulate Filter (cDPF)

Oxidation catalyst

Emission level
Water cooled EGR

Euro Stage V

TRANSMISSION

Transmission type:  
Ford MT82 manual 6-speed 
Ford 6R80 automatic 6-speed 

Gear ratios 


6th

5th

4th

3rd 

2nd

1st

Reverse

Final Drive (4x4)
0.794

0.691

1.000

0.867

1.223

1.143

1.721

1.521

2.839

2.342

5.441

4.171

4.935

3.400

3.55

3.73



Clutch
Hydraulically operated self-adjust clutch with dual mass flywheel
6-speed automatic transmission with manual Sport Mode, Brake Shift Interlock, Grade Control Logic (Automatic modes), Emergency downshift (Manual mode)

4x4 Transfer box
Two speed, right hand drop, single offset , aluminium shift-on-the-fly transfer box

4x4 ratios


1:1 (High Range)

2.48:1 (Low Range)

Max. speed for on-the-fly shifting
120 km/h

Dimensions and capacities

Exterior (mm)
Single Cab
Super Cab
Double Cab

Overall length
5274
5359
5359

Overall width
1850
1850
1850

Overall height max (empty vehicle)
1800 (1703)
1804
1815

Wheelbase
3220
3220
3220

Ground clearance
229
229
232

Wading depth (4x4)
800 (600)
800 (600)
800

Front tread (4x4)
1560 (1590)
1560
1560

Rear tread (4x4)
1560 (1590)
1560
1560

Front overhang
905
905
905

Rear overhang
1149
1226
1226

Angles (deg.)




Approach angle
n.a.
n.a.
27.7°

Departure angle
n.a.
n.a.
25.9°

Ramp angle 
n.a.
n.a.
24.4°

Interior (mm)




Front (mm)




Headroom
1024
1024
1022

Max. leg room 
1058
1058
1058

Shoulder room
1437
1437
1440

Rear (mm)




Headroom
-
938
975

Max. legroom
-
796
902

Shoulder room
-
1400
1430

Cargo Bed (mm)




Width
1544
1544
1544

Width between arches
1139
1139
1139

Length 
2317
1847
1560

Height
511
511
511

Loading height
835 (724)
835
835

Different figures for 4x2 versions in brackets.

Weights

Versions
Minimum kerbweight (kg)
Gross Vehicle Mass (kg)
Gross Payload 
(kg)
Max. towable mass (kg)

Single Cab





2.2L TDCi 150 PS 4x2
1791
2925
1134
2500 (750)







2.2L TDCi 150 PS 4x4
1891
3200
1309
3350 (750)







Super Cab





2.2L TDCi 150 PS 4x2
1835
2925
1090
2500 (750)







2.2L TDCi 150 PS 4x4
1946
3200
1254
3350 (750)







Double Cab





2.2L TDCi 150 PS 4x4
2048
3200
1152
3350 (750)







2.2L TDCi 150 PS 4x4 automatic
2063
3200
1137
3350 (750)







3.2L TDCi 200 PS 4x4
2073
3200
1127
3350 (750)







3.2L TDCi 200 PS 4x4 automatic
2083
3200
1117
3350 (750)







Minimum kerbweight represents the lightest kerbweight including full fluid levels and 90% fuel levels, subject to manufacturing tolerances and options, etc. fitted 

Towing limits quoted represent the maximum braked towing capacity of the vehicle on a 12 per cent gradient at sea level – unbraked towing capacities in brackets.

The performance and economy of all models will be reduced when used for towing.80 kg roof load for all versions.   220 kg tongue load for all versions.

Economy, Performance and Emissions


2.2 litre Duratorq TDCi
3.2 litre Duratorq TDCi 

Performance (PS)
150
200

Body Styles
all
all

Transmission Type
6-speed manual
6-speed automatic
6-speed manual
6-speed automatic

Euro Emissions Stage
Stage V
Stage V
Stage V
Stage V

CO2 Emissions (g/km)*
228 (219)
264
264
281

Urban fuel consumption*

l/100km (mpg)
27.4 (28.5)
22.6
23.0
21.6

Extra Urban fuel consumption l/100km (mpg)*
37.2 (38.7)
33.2
32.8
30.7

Combined fuel consumption l/100km (mpg)*
32.8 (34.0)
28.3
28.3
28.7

Max Speed km//h (mph)*
109 (103)
109
109
109

* Figures for 4x2 version in brackets. All CO2 emissions figures in g/km and fuel consumption figures are from officially approved tests in accordance with EC Directive 93/116/EC.  Fuel economy figures quoted are based on the European Fuel Economy Directive EU 80/1268/EEC and will differ from fuel economy drive cycle results in other regions of the world.Note: This information reflects preliminary specifications and was correct at the time of going to print. However, Ford policy is one of continuous product improvement. The right is reserved to change these details at any time.
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