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Vehicle Description
Technical Specification
Technical Specification
Technical Specification


Lotus Evora (IPS Option where stated)
Lotus Evora S (IPS Option where stated)
Lotus Evora GTE

Engine
Mid-mounted, transverse, 3456 cm3, 2GR-FE engine, aluminium lightweight and compact construction, V6 24 valve, water cooled, naturally aspirated with double overhead camshafts per cylinder bank, 4 valves per cylinder, Dual-Variable Valve Timing – intelligent, direct ignition system, electronic throttle control system-intelligent


Mid-mounted, transverse, 3456 cm3, 2GR-FE engine, aluminium lightweight and compact construction, V6 24 valve, water cooled, supercharged with double overhead camshafts per cylinder bank, 4 valves per cylinder, Dual-Variable Valve Timing – intelligent, direct ignition system, electronic throttle control system-intelligent

Harrop HTV 1320 supercharger assembly (utilising Eaton Twin Vortex Series (TVS) Technology ™)

Exhaust Protection Valve (opens at 4700 rpm) designed to reduce the back pressure at high rpm, allowing the engine to safely generate full power.
Mid-mounted, transverse, 3456 cm3, 2GR-FE engine, aluminium lightweight and compact construction, V6 24 valve, water cooled, supercharged with double overhead camshafts per cylinder bank, 4 valves per cylinder, Dual-Variable Valve Timing – intelligent, direct ignition system, electronic throttle control system-intelligent

Harrop HTV 1320 supercharger assembly (utilising Eaton Twin Vortex Series (TVS) Technology ™)

Compression ratio
10:1
10:1
10:1

Swept volume (Bore x Stroke)
94 x 83 mm
94 x 83 mm
94 x 83 mm

Engine management
Lotus T6e engine control unit
Lotus T6e engine control unit
Lotus T6e engine control unit

Max Power
280 PS / 206 kW / 276 hp @ 6400 rpm 
350 PS / 257.5 kW / 345 hp @ 7000 rpm
444 PS @ 7000 rpm

Max Torque
350 Nm / 258 lbft @ 4600rpm 
400 Nm / 295 lb ft @ 4500 rpm
420 Nm @ 4500 rpm

Emissions control
Three-way catalytic converter. 

Euro V emissions compliant with full On-Board Diagnostics (OBD).
Three-way catalytic converter

Euro V emissions compliant with full On-Board Diagnostics (OBD). 
Two way catalytic converter

Transmission
EA60 6 speed transverse Sports Ratios manual gearbox with open differential.

IPS: U660E 6 speed transverse automatic gearbox with open differential


EA60 6 speed transverse Sports Ratios manual gearbox with open differential 

IPS: U660E 6 speed transverse automatic gearbox with open differential


EA60 6 speed transverse Sports Ratios manual gearbox with open differential 

AMT Hydraulic Control unit

Suspension
Front and rear: Fully independent suspension, Forged Aluminium Double wishbone suspension, antiroll bar, Eibach springs and Bilstein dampers
Front and rear: Fully independent suspension, Forged Aluminium Double wishbone suspension, antiroll bar, Eibach springs and Bilstein dampers
Front and rear: Fully independent suspension, Double wishbone suspension, antiroll bar, Eibach springs and Bilstein dampers

Chassis
Lotus designed VVA (modular lightweight bonded Aluminium structure)

Total chassis weight 203 kg

Front module 29 kg

Rear module 58 kg

Chassis tub 116 kg

Whole vehicle torsional stiffness: 26,600 Nm per degree
Lotus designed VVA (modular lightweight bonded Aluminium structure)

Total chassis weight 203 kg

Front module 29 kg

Rear module 58 kg

Chassis tub 116 kg

Whole vehicle torsional stiffness: 26,600 Nm per degree
Lotus designed VVA (modular lightweight bonded Aluminium structure)

Total chassis weight 203 kg

Front module 29 kg

Rear module 58 kg

Chassis tub 116 kg

Whole vehicle torsional stiffness: 26,600 Nm per degree

Body
Lightweight composite body panels
Lightweight composite body panels
Lightweight carbon fibre body panels with composite front inspection panel and rear bootlid

Fuel Tank
Stainless steel fuel tank
Stainless steel fuel tank
Stainless steel fuel tank

Dynamic Performance Management (DPM)
Corner Brake Control (CBC)

Drag Torque Control (DTC)

Electronic Differential Lock (EDL)

Traction Control System (TCS)

Electronic Stability Control (ESC)

Anti-lock Braking System (ABS)*

Hydraulic Brake Assist (HBA)*

Electronic Brake Distribution (EBD)*

Understeer Recognition

All apart from * can be completely

switched off

DPM with Sports Mode button

Sport Mode increases the traction slip thresholds and removes understeer recognition, allowing the driver more vehicle control before an intervention is required.
Corner Brake Control (CBC)

Drag Torque Control (DTC)

Electronic Differential Lock (EDL)

Traction Control System (TCS)

Electronic Stability Control (ESC)

Anti-lock Braking System (ABS)*

Hydraulic Brake Assist (HBA)*

Electronic Brake Distribution (EBD)*

Understeer Recognition

All apart from * can be completely

switched off
DPM with Sports Mode button

Sport Mode increases the traction slip thresholds and removes understeer recognition, allowing the driver more vehicle control before an intervention is required.
Corner Brake Control (CBC)

Drag Torque Control (DTC)

Electronic Differential Lock (EDL)

Traction Control System (TCS)

Electronic Stability Control (ESC)

Anti-lock Braking System (ABS)*

Hydraulic Brake Assist (HBA)*

Electronic Brake Distribution (EBD)*

Understeer Recognition

All apart from * can be completely

switched off
DPM with Sports Mode button

Sport Mode increases the traction slip thresholds and removes understeer recognition, allowing the driver more vehicle control before an intervention is required.


Steering
Rack and pinion steering box with 2.86 turns lock-to-lock. Lotus tuned hydraulically assisted power assistance
Rack and pinion steering box with 2.86 turns lock-to-lock. Lotus tuned hydraulically assisted power assistance
Rack and pinion steering box with 2.86 turns lock-to-lock. Lotus tuned hydraulically assisted power assistance

Brakes

Servo-assisted, track tuned 4-channel Antilock Braking System (ABS)

Black AP-Racing four-piston calipers (front and rear) 

Front: 350 mm ventilated and cross drilled cast-iron discs
Rear: 332 mm ventilated and cross drilled cast-iron discs
Servo-assisted, track tuned 4-channel Antilock Braking System (ABS)

Black AP-Racing four-piston calipers (front and rear) 

Front: 350 mm ventilated and cross drilled cast-iron discs
Rear: 332 mm ventilated and cross drilled cast-iron discs

Wheels

Front

Rear
Cast wheels - Silver or Stealth Grey (option) – 18” x 8” front & 19” x 9.5” rear
Forged wheels (option):

Silver or Anthracite – 18” x 8” front & 19” x 9.5” rear - (3.2 kg lighter)

Diamond Cut “Turbine”

18” x 8” front & 19” x 9.5” rear
Diamond Cut “Design” 

19” front & 20” rear


Cast wheels – Silver or Stealth Grey – 18” x 8” front & 19” x 9.5” rear
Forged wheels (option):

Silver or Anthracite – 18” x 8” front & 19” x 9.5” rear - (3.2 kg lighter)

Diamond Cut “Turbine”

18” x 8” front & 19” x 9.5” rear
Diamond Cut “Design” 

19” front & 20” rear
Forged wheels:

Unique GTE centre lock

19” front & 20” rear

Tyres

Front

Rear
Standard:

225/40 ZR18 Pirelli P-Zero

255/35 ZR19 Pirelli P-Zero

Option

Bespoke Pirelli P-Zero Corsa (LS marking on tyres)

Front 235/35R19

Rear 275/30R20
Standard:

225/40 ZR18 Pirelli P-Zero

255/35 ZR19 Pirelli P-Zero

Option

Bespoke Pirelli P-Zero Corsa (LS marking on tyres)

Front 235/35R19

Rear 275/30R20
Bespoke Pirelli P-Zero Corsa (LS marking on tyres)

Front 235/35R19

Rear 275/30R20






Gear ratios

Manual
IPS
Manual
IPS
AMT


1st:
3.538
3.300
3.538
3.300
3.538


2nd:
1.913
1.900
1.913
1.900
1.913


3rd: 
1.407
1.420
1.407
1.420
1.407


4th: 
1.091
1.000
1.091
1.000
1.091


5th:
0.9697
0.713
0.9697
0.713
0.9697


6th:
0.8611
0.608
0.8611
0.608
0.8611


Reverse:
3.831
4.148
3.831
4.148
3.831


Final Drive (1st-4th):
3.777
3.685 (1st to 6th)
3.777
3.685 (1st to 6th)
3.777


Final Drive (5th – 6th)
3.238
N/A
3.238
N/A
3.238

Performance Figures




Max. Engine Speed
6600 rpm continuous and 68000 rpm transient

With Sports button activated

6800 rpm continuous and 7200 rpm transient 
6600 rpm continuous and 6800 rpm transient

With Sports button activated

6800 rpm continuous and 7200 rpm transient
7200 rpm 



0-60 mph
4.9 seconds

(with IPS option: 5.3 seconds)
4.6s
TBC

0-100 km/h
5.1 seconds

(with IPS option: 5.5 seconds)
4.8s
TBC

Maximum speed
261 km/h / 162 mph

(with IPS option: 250 km/h / 155 mph)
277 km/h / 172 mph
TBC

60-0 mph
33.6 meters – 2.4 seconds
33.6 meters – 2.4 seconds
TBC

100-0 mph
88.6 meters – 3.9 seconds
88.6 meters – 3.9 seconds
TBC

100-0 km/h
36.8 meters – 2.5 seconds
36.8 meters – 2.5 seconds
TBC

160-0 km/h
89.5 meters –  3.9 seconds
89.5 meters –  3.9 seconds
TBC

Fuel consumption – urban
21.5 mpg – 13.2 litres / 100km

(with IPS option: 21.2 mpg / – 13.3 litres / 100km
14.2 litres / 100km (19.9 mpg)

with IPS option: 19.6 mpg – 14.4 litres / 100km
TBC

Fuel consumption – extra urban
39.6 mpg – 7.1 litres / 100km

(with IPS option: 42.8 mpg – 6.6 litres / 100km
7.4 litres / 100km (38.4 mpg)

with IPS option: 40.8 mpg – 6.9 litres / 100km
TBC

Fuel consumption – combined
30.3 mpg – 9.3 litres / 100km

(with IPS option: 31.4 mpg – 9.0 litres / 100km
9.9 litres / 100km (28.7 mpg)

with IPS option: 29.3 mpg – 9.7 litres / 100km
TBC

CO2 emissions
217 g CO2  / km
(with IPS option: 210 g CO2  / km
CO2 Emissions 229 g CO2  / km

(with IPS option: 224 g CO2  / km)
TBC

Power to Weight
202 PS / tonne; with IPS option: 195 PS / tonne
243.5 PS / tonne; 
348 PS / tonne

Dimensions




Wheelbase
2574.5mm
2574.5mm
2574.5 mm

Track – front
1564 mm
1564mm
1664 mm

Track – rear
1575.5mm
1575.5mm
1685.5 mm

Overall length
4350.5mm
4360.5mm
4360.5mm

Overall width (door mirrors included)
1972mm
1972mm
1972 mm

Overall height – (unladen)
1229 mm
1229 mm
1214 mm

Overhang – front
1000 mm
1000 mm
1000 mm

Overhang – rear
776 mm
784 mm
784 mm

Turning circle
10.14 m
10.14 m
10.14 m

Ground clearance front– unladen
180.6 mm
180.6 mm
165.6 mm

Ground clearance between axels – unladen
140 mm
140 mm
125 mm

Vehicle mass – unladen (running order, full tank of fuel, no occupants, no luggage)
1382 kg

(With IPS option: 1436 kg)
1436 kg

(With IPS option: 1442 kg)
1276 kg

Luggage Capacity
50 kg
50 kg
50 kg

Weight distribution
Front: 39% 

Rear: 61% 
Front: 39% 

Rear: 61%
TBC

Drag Coefficient
0.33 (CdA: 0.627)
0.33 (CdA: 0.627)
TBC

Aerodynamic balance at 160 km/h (100 mph)
3 kg front; 5 kg rear
3 kg front; 5 kg rear
TBC

Fuel tank capacity
60 litres / 13.1 gallons usable volume
60 litres / 13.1 gallons usable volume
60 litres / 13.1 gallons usable volume

Boot capacity
160 litres
160 litres
~150 litres

Exterior Specification




Solid paint
S
S
Unique GTE Paint range

Metallic paint
O
O


Premium paint
O
O


Heated and electric door mirrors
S
S
S

Heated and electric (power-fold) door mirrors
O
O
S

Body coloured door handles
S
S
S

18” front and 19” rear cast alloy wheels
S
S
N/A

Interior Specification
Evora
Evora S
Evora GTE

Adjustable Recaro leather sports seats (front)
S
S
S with unique GTE styling

Heated front Recaro seats (standard with Premium Pack)
O
O
S

2+2 seat configuration with Isofix in rear
O
O
N / A

CD/MP3/WMA receiver
S
S
S

Central door locking
S
S
S

Flat bottomed magnesium steering wheel trimmed in leather
S
S
S (unique GTE styling)

Leather handbrake sleeve
S
S
S

Leather Gearknob
S
S
N / A

Manual steering column adjustment for length and height
S
S
S

Bespoke aluminium illuminated control knobs and switches
S
S
S

Electric windows
S
S
S

Remote release glove box
S
S
S

Door storage bins and integrated cup holders
S
S
S

12v interior accessory socket
S
S
S

12v boot mounted battery accessory socket
S
S
S

Lotus command centre with auxiliary trip computer and vehicle monitoring displays
S
S
S (unique GTE design)

Immobiliser and remote activated alarm
S
S
S

Safety Equipment




Dual Stage Driver and Passenger Airbags
S
S
S

Passenger Airbag on/off switch (non federal markets)
S
S
S

Load Limiting Pyrotechnic Pre-tensioning Front Seat Belts
S
S
S

ISOFIX Child Seat Anchorage (LATCH system in federal markets)
S
S
N / A

Options




SPORT PACK

Switchable sports mode with sharper throttle response, increased rpm limit and sports DPM setting

Sports diffuser

Titanium sports exhaust tailpipe

Cross-drilled brake discs

Red painted brake callipers
O
S
N / A 


PREMIUM PACK

Accent lighting

Premium floor mats

Leather door panelling below trim band

Leather trimmed door pockets, armrest, centre console and tailgate insert panel

Leather footwell side panels

Choice of seven leather shades:

Venom Red, Ebony Black, Cocoa Brown, Ash Grey, Imperial Blue, Cognac Brown, Ivory White

Heated front Recaro seats
O
O
N / A


PREMIUM PACK SUEDETEX®

Accent lighting

Premium floor mats

Leather door panelling below trim band

Leather trimmed door pockets, armrest, centre console and tailgate insert panel

Leather footwell side panels

Ebony Black leather and Slate Grey SuedeTex® 

Heated front Recaro seats
O
O
N / A

PREMIUM PACK SPORT

Accent lighting

Premium floor mats

Leather door panelling below trim band

Leather trimmed door pockets, armrest, centre console and tailgate insert panel

Leather footwell side panels

Choice of four leather shades:

Ebony Black with red contrast stitching and piping, Venom Red, Cocoa Brown and Imperial Blue with black contrast stitching and piping

Carbon effect leather inserts on front seats (and rear seats if 2+2)

Heated front Recaro seats




TECH PACK

Upgraded speakers and stereo system with 2x50W amplifier and subwoofer with dedicated amplifier, DVD player, 7” WVGA touch screen display

Bluetooth† mobile phone connection

USB connection for various iPod* models, MP3 players and memory sticks

Tyre pressure monitoring

Cruise control

Rear parking sensors
O
O
N / A

GTE PACK

Switchable sports mode with sharper throttle response, increased rpm limit and sports DPM setting

Unique GTE sports carbon fibre diffuser

Unique GTE exhaust tailpipe

Cross-drilled brake discs

Red painted brake callipers

Accent lighting

Carbon fibre floor panels

Unique carbon fibre interior door panels

Leather trimmed door pockets, armrest, centre console and tailgate insert panel

Carbon fibre footwell side panels

Heated front Recaro seats

Unique GTE trim

Heated front Recaro seats

Upgraded speakers and stereo system with 2x50W amplifier and subwoofer with dedicated amplifier, DVD player, 7” WVGA touch screen display

Bluetooth† mobile phone connection

USB connection for various iPod* models, MP3 players and memory sticks

Tyre pressure monitoring

Cruise control

Rear parking sensors
N/A
N/A
S

Interior Specification




Lotus Dynamic Performance Management (Lotus DPM)
S
S
S

Lotus tuned ABS system
S
S
S

Ventilated brake discs (350 mm front, 332 mm rear)
S
N/A
N/A

Servo assisted drilled ventilated discs (350 mm front, 332 mm rear)
O
S
S

AP Racing 4-piston calipers

(front and rear)
S
S
S

Classic wheel, silver, cast (18” front and 19” rear)
S
S
Forged wheels:

Unique GTE centre lock

19” front & 20” rear

Classic wheel, stealth grey, cast (18” front and 19” rear)
O
S


Sport wheel, silver or gloss anthracite, forged (18” front and 19” rear)
O
O


Design wheel, diamond cut, forged (19” front and 20” rear)
O
O


Design wheel, satin gunmetal or gloss black, forged (19” front and 20” rear)
O
O


Tyres

Pirelli P-Zero

Front 225/40 ZR18

Rear 255/35 ZR19
S
S
N / A

Tyres

Bespoke Pirelli P-Zero Corsa (LS marking on tyres)

Front 235/35R19

Rear 275/30R20
O
O
S

Sports rear diffuser
N/A
S
CARBON

Bi-Xenon headlights
S
S
S

Body coloured, electric door mirrors
S
O
CARBON

Black coloured, electric door mirrors
N/A
S
N / A

Power fold mirrors
O
O
S

Reversing Camera (only with tech pack)
O
O
S

Air conditioning
S
S
S

S = Standard

O = Optional

N/A = Not Available

POA = Price On Application.

iPod is a trade mark of Apple Inc registered in USA and other countries.

The Bluetooth word mark and logos are owned by Bluetooth SIG Inc
